{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["항목별 필요 시료량"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"항목별 필요 시료량","index":0,"n_rows":29,"n_cols":16,"rows_kept":29,"cut":false,"hidden":false,"merged":[[0,1,0,15],[2,4,11,4],[2,6,11,6],[2,7,11,7],[2,8,5,8],[2,10,5,10],[2,11,5,11],[6,10,7,10],[6,11,7,11],[8,10,9,10],[8,11,9,11],[12,4,28,4],[12,6,28,6],[12,7,28,7],[12,10,13,10],[12,11,13,11],[22,9,22,10]]}
[null,"KC 분석항목에 따른 필요 용출액량 계산기"]
[null,"시험재질(입력)\n('가~처', '전' 중 입력)","항목(자동입력됨)↓↓↓",null,null,"분석항목","필요시료량(mL)\n(입력필요)","자동입력",null,"분석항목","필요시료량(mL)\n(입력필요)","자동입력",null,null,"수도용 자재와 제품의 재질","위생안전기준 적용항목"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B3=$N$27, $P$27, B3=$N$3, $P$3, B3=$N$4, $P$4, B3=$N$5, $P$5, B3=$N$6, $P$6, B3=$N$7, $P$7, B3=$N$8, $P$8, B3=$N$9, $P$9, B3=$N$10, $P$10, B3=$N$11, $P$11, B3=$N$12, $P$12, B3=$N$13, $P$13, B3=$N$14, $P$14, B3=$N$15, $P$15, B3=$N$16, $P$16, B3=$N$17, $P$17, B3=$N$18, $P$18, B3=$N$19, $P$19, B3=$N$20, $P$20, B3=$N$21, $P$21, B3=$N$22, $P$22, B3=$N$23, $P$23, B3=$N$24, $P$24, B3=$N$25, $P$25, B3=$N$26, $P$26), \"\")","v":""},null,"금\n속\n류","비소",100,{"$f":"IF(COUNT(FIND($F4,C$26),FIND($F5,C$26),FIND($F6,C$26),FIND($F7,C$26),FIND($F8,C$26),FIND($F9,C$26),FIND($F10,C$26),FIND($F11,C$26),FIND($F12,C$26),FIND($F3,C$26))>0,$G$3,0)","v":0},"이\n온\n류","불소",50,{"$f":"IF(COUNT(FIND($J3,C$26),FIND($J4,C$26),FIND($J5,C$26),FIND($J6,C$26))>0,$K$3,0)","v":0},null,"가","가. 구리나 구리합금 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  아연,  철,  수은,  니켈"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B4=$N$27, $P$27, B4=$N$3, $P$3, B4=$N$4, $P$4, B4=$N$5, $P$5, B4=$N$6, $P$6, B4=$N$7, $P$7, B4=$N$8, $P$8, B4=$N$9, $P$9, B4=$N$10, $P$10, B4=$N$11, $P$11, B4=$N$12, $P$12, B4=$N$13, $P$13, B4=$N$14, $P$14, B4=$N$15, $P$15, B4=$N$16, $P$16, B4=$N$17, $P$17, B4=$N$18, $P$18, B4=$N$19, $P$19, B4=$N$20, $P$20, B4=$N$21, $P$21, B4=$N$22, $P$22, B4=$N$23, $P$23, B4=$N$24, $P$24, B4=$N$25, $P$25, B4=$N$26, $P$26), \"\")","v":""},null,null,"카드뮴",null,null,null,"질산성질소",null,null,null,"나","나. 스테인리스 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  아연,  수은,  니켈"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B5=$N$27, $P$27, B5=$N$3, $P$3, B5=$N$4, $P$4, B5=$N$5, $P$5, B5=$N$6, $P$6, B5=$N$7, $P$7, B5=$N$8, $P$8, B5=$N$9, $P$9, B5=$N$10, $P$10, B5=$N$11, $P$11, B5=$N$12, $P$12, B5=$N$13, $P$13, B5=$N$14, $P$14, B5=$N$15, $P$15, B5=$N$16, $P$16, B5=$N$17, $P$17, B5=$N$18, $P$18, B5=$N$19, $P$19, B5=$N$20, $P$20, B5=$N$21, $P$21, B5=$N$22, $P$22, B5=$N$23, $P$23, B5=$N$24, $P$24, B5=$N$25, $P$25, B5=$N$26, $P$26), \"\")","v":""},null,null,"구리",null,null,null,"아질산성질소",null,null,null,"다","다. 주철 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  아연,  수은,  니켈"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B6=$N$27, $P$27, B6=$N$3, $P$3, B6=$N$4, $P$4, B6=$N$5, $P$5, B6=$N$6, $P$6, B6=$N$7, $P$7, B6=$N$8, $P$8, B6=$N$9, $P$9, B6=$N$10, $P$10, B6=$N$11, $P$11, B6=$N$12, $P$12, B6=$N$13, $P$13, B6=$N$14, $P$14, B6=$N$15, $P$15, B6=$N$16, $P$16, B6=$N$17, $P$17, B6=$N$18, $P$18, B6=$N$19, $P$19, B6=$N$20, $P$20, B6=$N$21, $P$21, B6=$N$22, $P$22, B6=$N$23, $P$23, B6=$N$24, $P$24, B6=$N$25, $P$25, B6=$N$26, $P$26), \"\")","v":""},null,null,"납",null,null,null,"염소이온",null,null,null,"라","라. 아연도금 또는 아연도금강 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  아연,  철,  수은,  니켈"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B7=$N$27, $P$27, B7=$N$3, $P$3, B7=$N$4, $P$4, B7=$N$5, $P$5, B7=$N$6, $P$6, B7=$N$7, $P$7, B7=$N$8, $P$8, B7=$N$9, $P$9, B7=$N$10, $P$10, B7=$N$11, $P$11, B7=$N$12, $P$12, B7=$N$13, $P$13, B7=$N$14, $P$14, B7=$N$15, $P$15, B7=$N$16, $P$16, B7=$N$17, $P$17, B7=$N$18, $P$18, B7=$N$19, $P$19, B7=$N$20, $P$20, B7=$N$21, $P$21, B7=$N$22, $P$22, B7=$N$23, $P$23, B7=$N$24, $P$24, B7=$N$25, $P$25, B7=$N$26, $P$26), \"\")","v":""},null,null,"셀레늄",null,null,null,"맛",200,{"$f":"IF(COUNT(FIND($J7,C$26),FIND($J8,C$26))>0,$K$7,0)","v":0},null,"마","마. 폴리에틸렌 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B8=$N$27, $P$27, B8=$N$3, $P$3, B8=$N$4, $P$4, B8=$N$5, $P$5, B8=$N$6, $P$6, B8=$N$7, $P$7, B8=$N$8, $P$8, B8=$N$9, $P$9, B8=$N$10, $P$10, B8=$N$11, $P$11, B8=$N$12, $P$12, B8=$N$13, $P$13, B8=$N$14, $P$14, B8=$N$15, $P$15, B8=$N$16, $P$16, B8=$N$17, $P$17, B8=$N$18, $P$18, B8=$N$19, $P$19, B8=$N$20, $P$20, B8=$N$21, $P$21, B8=$N$22, $P$22, B8=$N$23, $P$23, B8=$N$24, $P$24, B8=$N$25, $P$25, B8=$N$26, $P$26), \"\")","v":""},null,null,"아연",null,null,null,"냄새",null,null,null,"바","바. 폴리프로필렌 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B9=$N$27, $P$27, B9=$N$3, $P$3, B9=$N$4, $P$4, B9=$N$5, $P$5, B9=$N$6, $P$6, B9=$N$7, $P$7, B9=$N$8, $P$8, B9=$N$9, $P$9, B9=$N$10, $P$10, B9=$N$11, $P$11, B9=$N$12, $P$12, B9=$N$13, $P$13, B9=$N$14, $P$14, B9=$N$15, $P$15, B9=$N$16, $P$16, B9=$N$17, $P$17, B9=$N$18, $P$18, B9=$N$19, $P$19, B9=$N$20, $P$20, B9=$N$21, $P$21, B9=$N$22, $P$22, B9=$N$23, $P$23, B9=$N$24, $P$24, B9=$N$25, $P$25, B9=$N$26, $P$26), \"\")","v":""},null,null,"철",null,null,null,"색도",130,{"$f":"IF(COUNT(FIND($J9,C$26),FIND($J10,C$26))>0,$K$9,0)","v":0},null,"사","사. 폴리부틸렌 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B10=$N$27, $P$27, B10=$N$3, $P$3, B10=$N$4, $P$4, B10=$N$5, $P$5, B10=$N$6, $P$6, B10=$N$7, $P$7, B10=$N$8, $P$8, B10=$N$9, $P$9, B10=$N$10, $P$10, B10=$N$11, $P$11, B10=$N$12, $P$12, B10=$N$13, $P$13, B10=$N$14, $P$14, B10=$N$15, $P$15, B10=$N$16, $P$16, B10=$N$17, $P$17, B10=$N$18, $P$18, B10=$N$19, $P$19, B10=$N$20, $P$20, B10=$N$21, $P$21, B10=$N$22, $P$22, B10=$N$23, $P$23, B10=$N$24, $P$24, B10=$N$25, $P$25, B10=$N$26, $P$26), \"\")","v":""},null,null,"니켈",null,null,null,"탁도",null,null,null,"아","아. 폴리염화비닐 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B11=$N$27, $P$27, B11=$N$3, $P$3, B11=$N$4, $P$4, B11=$N$5, $P$5, B11=$N$6, $P$6, B11=$N$7, $P$7, B11=$N$8, $P$8, B11=$N$9, $P$9, B11=$N$10, $P$10, B11=$N$11, $P$11, B11=$N$12, $P$12, B11=$N$13, $P$13, B11=$N$14, $P$14, B11=$N$15, $P$15, B11=$N$16, $P$16, B11=$N$17, $P$17, B11=$N$18, $P$18, B11=$N$19, $P$19, B11=$N$20, $P$20, B11=$N$21, $P$21, B11=$N$22, $P$22, B11=$N$23, $P$23, B11=$N$24, $P$24, B11=$N$25, $P$25, B11=$N$26, $P$26), \"\")","v":""},null,null,"망간",null,null,null,"시안",20,{"$f":"IFERROR(COUNT(FIND($J11,C$26)),\"\")*K11","v":0},null,"자","자. 폴리아미드 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B12=$N$27, $P$27, B12=$N$3, $P$3, B12=$N$4, $P$4, B12=$N$5, $P$5, B12=$N$6, $P$6, B12=$N$7, $P$7, B12=$N$8, $P$8, B12=$N$9, $P$9, B12=$N$10, $P$10, B12=$N$11, $P$11, B12=$N$12, $P$12, B12=$N$13, $P$13, B12=$N$14, $P$14, B12=$N$15, $P$15, B12=$N$16, $P$16, B12=$N$17, $P$17, B12=$N$18, $P$18, B12=$N$19, $P$19, B12=$N$20, $P$20, B12=$N$21, $P$21, B12=$N$22, $P$22, B12=$N$23, $P$23, B12=$N$24, $P$24, B12=$N$25, $P$25, B12=$N$26, $P$26), \"\")","v":""},null,null,"나트륨",null,null,null,"음이온계면활성제",20,0,null,"차","차. 폴리술폰 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B13=$N$27, $P$27, B13=$N$3, $P$3, B13=$N$4, $P$4, B13=$N$5, $P$5, B13=$N$6, $P$6, B13=$N$7, $P$7, B13=$N$8, $P$8, B13=$N$9, $P$9, B13=$N$10, $P$10, B13=$N$11, $P$11, B13=$N$12, $P$12, B13=$N$13, $P$13, B13=$N$14, $P$14, B13=$N$15, $P$15, B13=$N$16, $P$16, B13=$N$17, $P$17, B13=$N$18, $P$18, B13=$N$19, $P$19, B13=$N$20, $P$20, B13=$N$21, $P$21, B13=$N$22, $P$22, B13=$N$23, $P$23, B13=$N$24, $P$24, B13=$N$25, $P$25, B13=$N$26, $P$26), \"\")","v":""},null,"V\nO\nC\ns","VOCs",100,{"$f":"IF(COUNT(FIND($F14,C$26),FIND($F15,C$26),FIND($F16,C$26),FIND($F17,C$26),FIND($F18,C$26),FIND($F19,C$26),FIND($F20,C$26),FIND($F21,C$26),FIND($F22,C$26),FIND($F23,C$26),FIND($F24,C$26),FIND($F25,C$26),FIND($F26,C$26),FIND($F27,C$26),FIND($F28,C$26),FIND($F29,C$26),FIND($F13,C$26))>0,$G$13,0)","v":0},null,"2,4-톨루엔디아민",500,{"$f":"IF(COUNT(FIND($J13,C$26),FIND($J14,C$26))>0,$K$13,0)","v":0},null,"카","카. ABS 수지(아크릴로니트릴, 부타디엔, 스티렌) 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B14=$N$27, $P$27, B14=$N$3, $P$3, B14=$N$4, $P$4, B14=$N$5, $P$5, B14=$N$6, $P$6, B14=$N$7, $P$7, B14=$N$8, $P$8, B14=$N$9, $P$9, B14=$N$10, $P$10, B14=$N$11, $P$11, B14=$N$12, $P$12, B14=$N$13, $P$13, B14=$N$14, $P$14, B14=$N$15, $P$15, B14=$N$16, $P$16, B14=$N$17, $P$17, B14=$N$18, $P$18, B14=$N$19, $P$19, B14=$N$20, $P$20, B14=$N$21, $P$21, B14=$N$22, $P$22, B14=$N$23, $P$23, B14=$N$24, $P$24, B14=$N$25, $P$25, B14=$N$26, $P$26), \"\")","v":""},null,null,"사염화탄소",null,null,null,"2,6-톨루엔디아민",null,null,null,"타","타. 폴리옥시메틸렌 또는 폴리포름알데히드 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량,  포름알데히드"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B15=$N$27, $P$27, B15=$N$3, $P$3, B15=$N$4, $P$4, B15=$N$5, $P$5, B15=$N$6, $P$6, B15=$N$7, $P$7, B15=$N$8, $P$8, B15=$N$9, $P$9, B15=$N$10, $P$10, B15=$N$11, $P$11, B15=$N$12, $P$12, B15=$N$13, $P$13, B15=$N$14, $P$14, B15=$N$15, $P$15, B15=$N$16, $P$16, B15=$N$17, $P$17, B15=$N$18, $P$18, B15=$N$19, $P$19, B15=$N$20, $P$20, B15=$N$21, $P$21, B15=$N$22, $P$22, B15=$N$23, $P$23, B15=$N$24, $P$24, B15=$N$25, $P$25, B15=$N$26, $P$26), \"\")","v":""},null,null,"1,2-디클로로에탄",null,null,null,"6가크롬",50,{"$f":"IFERROR(COUNT(FIND($J15,C$26)),\"\")*K15","v":0},null,"파","파. 에보나이트 재질이거나 에보나이트로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  니켈,  페놀류,  과망간산칼륨소비량,  포름알데히드,  수은"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B16=$N$27, $P$27, B16=$N$3, $P$3, B16=$N$4, $P$4, B16=$N$5, $P$5, B16=$N$6, $P$6, B16=$N$7, $P$7, B16=$N$8, $P$8, B16=$N$9, $P$9, B16=$N$10, $P$10, B16=$N$11, $P$11, B16=$N$12, $P$12, B16=$N$13, $P$13, B16=$N$14, $P$14, B16=$N$15, $P$15, B16=$N$16, $P$16, B16=$N$17, $P$17, B16=$N$18, $P$18, B16=$N$19, $P$19, B16=$N$20, $P$20, B16=$N$21, $P$21, B16=$N$22, $P$22, B16=$N$23, $P$23, B16=$N$24, $P$24, B16=$N$25, $P$25, B16=$N$26, $P$26), \"\")","v":""},null,null,"1,1-디클로로에틸렌",null,null,null,"수은",20,0,null,"하","하. 에폭시 수지 재질이거나 에폭시 수지로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  페놀류,  시안,  과망간산칼륨소비량,  아민류,  2,4-톨루엔디아민,  2,6-톨루엔디아민"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B17=$N$27, $P$27, B17=$N$3, $P$3, B17=$N$4, $P$4, B17=$N$5, $P$5, B17=$N$6, $P$6, B17=$N$7, $P$7, B17=$N$8, $P$8, B17=$N$9, $P$9, B17=$N$10, $P$10, B17=$N$11, $P$11, B17=$N$12, $P$12, B17=$N$13, $P$13, B17=$N$14, $P$14, B17=$N$15, $P$15, B17=$N$16, $P$16, B17=$N$17, $P$17, B17=$N$18, $P$18, B17=$N$19, $P$19, B17=$N$20, $P$20, B17=$N$21, $P$21, B17=$N$22, $P$22, B17=$N$23, $P$23, B17=$N$24, $P$24, B17=$N$25, $P$25, B17=$N$26, $P$26), \"\")","v":""},null,null,"1,1,2-트리클로로에탄",null,null,null,"페놀류",200,0,null,"거","거. 아크릴 수지 재질이거나 아크릴 수지로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  수은,  VOCs,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B18=$N$27, $P$27, B18=$N$3, $P$3, B18=$N$4, $P$4, B18=$N$5, $P$5, B18=$N$6, $P$6, B18=$N$7, $P$7, B18=$N$8, $P$8, B18=$N$9, $P$9, B18=$N$10, $P$10, B18=$N$11, $P$11, B18=$N$12, $P$12, B18=$N$13, $P$13, B18=$N$14, $P$14, B18=$N$15, $P$15, B18=$N$16, $P$16, B18=$N$17, $P$17, B18=$N$18, $P$18, B18=$N$19, $P$19, B18=$N$20, $P$20, B18=$N$21, $P$21, B18=$N$22, $P$22, B18=$N$23, $P$23, B18=$N$24, $P$24, B18=$N$25, $P$25, B18=$N$26, $P$26), \"\")","v":""},null,null,"트리클로로에틸렌",null,null,null,"과망간산칼륨소비량",100,0,null,"너","너. 폴리우레탄 재질이거나 폴리우레탄으로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  수은,  VOCs,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B19=$N$27, $P$27, B19=$N$3, $P$3, B19=$N$4, $P$4, B19=$N$5, $P$5, B19=$N$6, $P$6, B19=$N$7, $P$7, B19=$N$8, $P$8, B19=$N$9, $P$9, B19=$N$10, $P$10, B19=$N$11, $P$11, B19=$N$12, $P$12, B19=$N$13, $P$13, B19=$N$14, $P$14, B19=$N$15, $P$15, B19=$N$16, $P$16, B19=$N$17, $P$17, B19=$N$18, $P$18, B19=$N$19, $P$19, B19=$N$20, $P$20, B19=$N$21, $P$21, B19=$N$22, $P$22, B19=$N$23, $P$23, B19=$N$24, $P$24, B19=$N$25, $P$25, B19=$N$26, $P$26), \"\")","v":""},null,null,"벤젠",null,null,null,"포름알데히드",100,0,null,"더","더. 실리콘 재질이거나 실리콘으로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  수은,  VOCs,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B20=$N$27, $P$27, B20=$N$3, $P$3, B20=$N$4, $P$4, B20=$N$5, $P$5, B20=$N$6, $P$6, B20=$N$7, $P$7, B20=$N$8, $P$8, B20=$N$9, $P$9, B20=$N$10, $P$10, B20=$N$11, $P$11, B20=$N$12, $P$12, B20=$N$13, $P$13, B20=$N$14, $P$14, B20=$N$15, $P$15, B20=$N$16, $P$16, B20=$N$17, $P$17, B20=$N$18, $P$18, B20=$N$19, $P$19, B20=$N$20, $P$20, B20=$N$21, $P$21, B20=$N$22, $P$22, B20=$N$23, $P$23, B20=$N$24, $P$24, B20=$N$25, $P$25, B20=$N$26, $P$26), \"\")","v":""},null,null,"1,1,1-트리클로로에탄",null,null,null,"아민류",200,0,null,"러","러. 폴리에스테르 재질이거나 폴리에스테르로 도장된 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  수은,  VOCs,  과망간산칼륨소비량"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B21=$N$27, $P$27, B21=$N$3, $P$3, B21=$N$4, $P$4, B21=$N$5, $P$5, B21=$N$6, $P$6, B21=$N$7, $P$7, B21=$N$8, $P$8, B21=$N$9, $P$9, B21=$N$10, $P$10, B21=$N$11, $P$11, B21=$N$12, $P$12, B21=$N$13, $P$13, B21=$N$14, $P$14, B21=$N$15, $P$15, B21=$N$16, $P$16, B21=$N$17, $P$17, B21=$N$18, $P$18, B21=$N$19, $P$19, B21=$N$20, $P$20, B21=$N$21, $P$21, B21=$N$22, $P$22, B21=$N$23, $P$23, B21=$N$24, $P$24, B21=$N$25, $P$25, B21=$N$26, $P$26), \"\")","v":""},null,null,"디클로로메탄",null,null,null,"증발잔류물",200,0,null,"머","머. 에틸렌고무, 프로필렌고무 또는 디엔고무 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  페놀류"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B22=$N$27, $P$27, B22=$N$3, $P$3, B22=$N$4, $P$4, B22=$N$5, $P$5, B22=$N$6, $P$6, B22=$N$7, $P$7, B22=$N$8, $P$8, B22=$N$9, $P$9, B22=$N$10, $P$10, B22=$N$11, $P$11, B22=$N$12, $P$12, B22=$N$13, $P$13, B22=$N$14, $P$14, B22=$N$15, $P$15, B22=$N$16, $P$16, B22=$N$17, $P$17, B22=$N$18, $P$18, B22=$N$19, $P$19, B22=$N$20, $P$20, B22=$N$21, $P$21, B22=$N$22, $P$22, B22=$N$23, $P$23, B22=$N$24, $P$24, B22=$N$25, $P$25, B22=$N$26, $P$26), \"\")","v":""},null,null,"시스-1,2-디클로로에틸렌",null,null,null,"잔류염소의감량",20,0,null,"버","버. 아크릴로니트릴부타디엔고무 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  페놀류"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B23=$N$27, $P$27, B23=$N$3, $P$3, B23=$N$4, $P$4, B23=$N$5, $P$5, B23=$N$6, $P$6, B23=$N$7, $P$7, B23=$N$8, $P$8, B23=$N$9, $P$9, B23=$N$10, $P$10, B23=$N$11, $P$11, B23=$N$12, $P$12, B23=$N$13, $P$13, B23=$N$14, $P$14, B23=$N$15, $P$15, B23=$N$16, $P$16, B23=$N$17, $P$17, B23=$N$18, $P$18, B23=$N$19, $P$19, B23=$N$20, $P$20, B23=$N$21, $P$21, B23=$N$22, $P$22, B23=$N$23, $P$23, B23=$N$24, $P$24, B23=$N$25, $P$25, B23=$N$26, $P$26), \"\")","v":""},null,null,"테트라클로로에틸렌",null,null,null,"합",null,{"$f":"SUM(H3:H29,L3:L22)","v":0},null,"서","서. 스티렌부타디엔고무 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  페놀류"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B24=$N$27, $P$27, B24=$N$3, $P$3, B24=$N$4, $P$4, B24=$N$5, $P$5, B24=$N$6, $P$6, B24=$N$7, $P$7, B24=$N$8, $P$8, B24=$N$9, $P$9, B24=$N$10, $P$10, B24=$N$11, $P$11, B24=$N$12, $P$12, B24=$N$13, $P$13, B24=$N$14, $P$14, B24=$N$15, $P$15, B24=$N$16, $P$16, B24=$N$17, $P$17, B24=$N$18, $P$18, B24=$N$19, $P$19, B24=$N$20, $P$20, B24=$N$21, $P$21, B24=$N$22, $P$22, B24=$N$23, $P$23, B24=$N$24, $P$24, B24=$N$25, $P$25, B24=$N$26, $P$26), \"\")","v":""},null,null,"에피클로로히드린",null,null,null,null,null,null,null,"어","어. 불소고무 재질의 수도용 자재와 제품","맛,  냄새,  색도,  탁도,  VOCs,  페놀류,  불소"]
[null,null,{"$f":"IFERROR(_xlfn.IFS(B25=$N$27, $P$27, B25=$N$3, $P$3, B25=$N$4, $P$4, B25=$N$5, $P$5, B25=$N$6, $P$6, B25=$N$7, $P$7, B25=$N$8, $P$8, B25=$N$9, $P$9, B25=$N$10, $P$10, B25=$N$11, $P$11, B25=$N$12, $P$12, B25=$N$13, $P$13, B25=$N$14, $P$14, B25=$N$15, $P$15, B25=$N$16, $P$16, B25=$N$17, $P$17, B25=$N$18, $P$18, B25=$N$19, $P$19, B25=$N$20, $P$20, B25=$N$21, $P$21, B25=$N$22, $P$22, B25=$N$23, $P$23, B25=$N$24, $P$24, B25=$N$25, $P$25, B25=$N$26, $P$26), \"\")","v":""},null,null," 아세트산비닐",null,null,null,null,null,null,null,"저","저. 아스팔트 재질의 수도용 자재 와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  망간,  수은,  니켈,  VOCs"]
[null,{"$f":"RemoveDupes2(B3&\",\"&B4&\",\"&B5&\",\"&B6&\",\"&B7&\",\"&B8&\",\"&B9&\",\"&B10&\",\"&B11&\",\"&B12&\",\"&B13&\",\"&B14&\",\"&B15&\",\"&B16&\",\"&B17&\",\"&B18&\",\"&B19&\",\"&B20&\",\"&B21&\",\"&B22&\",\"&B23&\",\"&B24&\",\"&B25, \",\")","v":""},{"$f":"RemoveDupes2(C3&\", \"&C4&\", \"&C5&\", \"&C6&\", \"&C7&\", \"&C8&\", \"&C9&\", \"&C10&\", \"&C11&\", \"&C12&\", \"&C13&\", \"&C14&\", \"&C15&\", \"&C16&\", \"&C17&\", \"&C18&\", \"&C19&\", \"&C20&\", \"&C21&\", \"&C22&\", \"&C23&\", \"&C24&\", \"&C25, \", \")","v":""},null,null,"스티렌",null,null,null,null,null,null,null,"처","처. 시멘트 재질의 수도용 자재 와 제품","맛,  냄새,  색도,  탁도,  비소,  카드뮴,  6가크롬,  구리,  납,  셀레늄,  수은,  니켈"]
[null,"필요 시료량(mL)",{"$f":"L23","v":0},null,null,"1,2-부타디엔",null,null,null,null,null,null,null,"전","전항목(그 밖에)","맛, 냄새, 색도, 탁도, 비소, 카드뮴, 구리, 납, 셀레늄, 아연, 철, 니켈, 망간, 6가크롬, 수은, 사염화탄소, 1,2-디클로로에탄, 1,1-디클로로에틸렌, 1,1,2-트리클로로에탄, 트리클로로에틸렌, 벤젠, 1,1,1-트리클로로에탄, 디클로로메탄, 시스-1,2-디클로로에틸렌, 테트라클로로에틸렌, 에피클로로히드린, 아세트산비닐, 스티렌, 1,2-부타디엔, 1,3-부타디엔, N,N-디메틸아닐린, 페놀류, 과망간산칼륨소비량, 포름알데히드, 시안, 아민류, 2,4-톨루엔디아민, 2,6-톨루엔디아민, 불소, 질산성질소, 아질산성질소, 염소이온, 나트륨, 증발잔류물, 음이온계면활성제, 잔류염소의감량"]
[null,null,null,null,null,"1,3-부타디엔"]
[null,null,null,null,null,"N,N-디메틸아닐린"]